**Signal Design In The Presence of Laser Phase Noise**

Signal design strategies to improve phase noise tolerance of a short-range coherent system such as 400ZR and beyond. We propose a low-complexity approach demonstrating up to .7dB gains (both GMI and post-FEC) when compared to 16QAM constellations and 0.4dB for AWGN optimal formats.